{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":7,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RX-KM"]
[]
[]
[]
[]
["","","","","","RX25KMV1B","RX35KMV1B"]
["Dimensions","Unit","","Height","mm","550","550"]
["","","","Width","mm","675","675"]
["","","","Depth","mm","284","284"]
["Weight","Unit","","","kg","24","28"]
["Compressor","Type","","","","Hermetically sealed swing compressor","Hermetically sealed swing compressor"]
["Operation range","Cooling","Ambient","Min.","°CDB","10 (1)","10 (1)"]
["","","","Max.","°CDB","46","46"]
["","Heating","Ambient","Min.","°CWB","-15","-15"]
["","","","Max.","°CWB","18","18"]
["Sound pressure level","Cooling","","High","dBA","46","48"]
["","Heating","","High","dBA","47","48"]
["Refrigerant","Type","","","","R-410A","R-410A"]
["","Charge","","","kg","0.70","0.94"]
["","Charge","","","tCO2Eq","1.5","2.1"]
["","GWP","","","","2087.5","2087.5"]
["Piping connections","Piping length","OU - IU","Max.","m","15","15"]
["","Additional refrigerant charge","","","kg/m","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)"]
["","Level difference","IU - OU","Max.","m","12","12"]
["Standard Accessories","Installation manual","","","","1","1"]
["","Refrigerant charge label","","","","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1"]
["","Drain plug (only heat pump models)","","","","1","1"]
["","Drain cap","","","","6","6"]
["Power supply","Phase","","","","1~","1~"]
["","Frequency","","","Hz","50","50"]
["","Voltage","","","V","220-240","220-240"]
["Notes","","","","","(1) - Operation range in combination with FTX-J3: min. 10°CDB ~ max. 46°CDB","(1) - Operation range in combination with FTX-J3: min. 10°CDB ~ max. 46°CDB"]