{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":61,"n_cols":9,"rows_kept":61,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXG-L"]
[]
[]
[]
[]
["","","","","","RXG20L2V1B","RXG25L2V1B","RXG35L2V1B","RXG50L2V1B"]
["Sound pressure level","Heating","","High","dBA","","47","48"]
["","Cooling","","High","dBA","","46","48"]
["Standard Accessories","Joint (drain)","","","","1","1","1","1"]
["","Installation manual","","","","1","1","1","1"]
["Refrigerant","Charge","","","TCO2Eq","","2.2","2.2"]
["","GWP","","","","","2,087.5","2,087.5"]
["","Charge","","","kg","","1.05","1.05"]
["","Type","","","","","R-410A","R-410A"]
["Fan motor","Speed","Cooling","Super low","rpm","","780","780"]
["","","Heating","Super low","rpm","","740","740"]
["Piping connections","Level difference","IU - OU","Max.","m","","15","15"]
["","Additional refrigerant charge","","","kg/m","","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)"]
["Dimensions","Unit","","Width","mm","","765","765"]
["","","","Depth","mm","","285","285"]
["","","","Height","mm","","550","550"]
["Compressor","Type","","","","","Hermetically sealed swing compressor","Hermetically sealed swing compressor"]
["Weight","Unit","","","kg","","35","35"]
["Fan","Air flow rate","Heating","Super low","cfm","","932","932"]
["","","Cooling","Super low","cfm","","1,094","1,094"]
["Power supply","Phase","","","","","1~","1~"]
["","Frequency","","","Hz","","50","50"]
["","Voltage","","","V","","220-240","220-240"]
["Notes","","","","","(1) - 220V","(1) - SL: The silent fan level of the air flow rate setting","(1) - SL: The silent fan level of the air flow rate setting","(1) - 220V"]
["","","","","","(2) - 230V","(2) - 220V","(2) - 220V","(2) - 230V"]
["","","","","","(3) - 240V","(3) - 230V","(3) - 230V","(3) - 240V"]
["","","","","","(4) - Operation range in combination with Nexura, FVXG-K, cooling: min. 10°CDB - max. 46°CDB; heating: min. -15°CWB - max. 18°CWB","(4) - 240V","(4) - 240V","(4) - Operation range in combination with Nexura, FVXG-K, cooling: min. 10°CDB - max. 46°CDB; heating: min. -15°CWB - max. 18°CWB"]
["","","","","","","(5) - Operation range in combination with Nexura, FVXG-K, cooling: min. 10°CDB - max. 46°CDB; heating: min. -15°CWB - max. 18°CWB","(5) - Operation range in combination with Nexura, FVXG-K, cooling: min. 10°CDB - max. 46°CDB; heating: min. -15°CWB - max. 18°CWB"]
["","","","","","","(6) - Contains fluorinated greenhouse gases","(6) - Contains fluorinated greenhouse gases"]
["Fan","Air flow rate","Cooling","Super low","m³/min","31.0","","","42.6"]
["","","Heating","Super low","m³/min","26.4","","","38.3"]
["","","","Super low","cfm","1094","","","1504"]
["","","Heating","Super low","cfm","932","","","1352"]
["Dimensions","Unit","","Height","mm","550","","","735"]
["","","","Width","mm","765","","","825"]
["","","","Depth","mm","285","","","300"]
["Weight","Unit","","","kg","35","","","48"]
["Fan motor","Speed","Cooling","Super low","rpm","780","","","670"]
["","","Heating","Super low","rpm","740","","","670"]
["Compressor","Type","","","","Hermetically sealed swing compressor","","","Hermetically sealed swing compressor"]
["Operation range","Cooling","Ambient","Min.","°CDB","-10 (5)","","","-10 (5)"]
["","","","Max.","°CDB","46","","","46"]
["","Heating","Ambient","Min.","°CWB","-15","","","-15"]
["","","","Max.","°CWB","18","","","18"]
["Sound pressure level","Cooling","","High","dBA","46","","","48"]
["","Heating","","High","dBA","47","","","48"]
["Refrigerant","Type","","","","R-410A","","","R-410A"]
["","Charge","","","kg","1.05","","","1.6"]
["","Charge","","","tCO2Eq","2.2","","","3.3"]
["","GWP","","","","2087.5","","","2087.5"]
["Piping connections","Piping length","OU - IU","Max.","m","20","","","30"]
["","Additional refrigerant charge","","","kg/m","0.02 (for piping length exceeding 10m)","","","0.02 (for piping length exceeding 10m)"]
["","Level difference","IU - OU","Max.","m","15","","","20"]
["Power supply","Phase","","","","1~","","","1~"]
["","Frequency","","","Hz","50","","","50"]
["","Voltage","","","V","220-240","","","220-240"]