{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":112,"n_cols":6,"rows_kept":112,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXYN-B"]
[]
[]
[]
[]
["","","","","","RXYN10B7Y1B"]
["Recommended combination","","","","","4 x FXSN63B2VEB"]
["Recommended combination 2","","","","","4 x FXFN63B2VEB"]
["Cooling capacity","Prated,c","","","kW","28.0 (1)"]
["Heating capacity","Prated,h","","","kW","28.0 (2)"]
["","Nom.","","6°CWB","kW","28.00 (2)"]
["COP at nom. capacity","6°CWB","","","KW/KW","294.00 (2)"]
["SEER","","","","","4.80"]
["SEER recommended combination 2","","","","","4.80"]
["SCOP","","","","","3.50"]
["SCOP recommended combination 2","","","","","3.50"]
["Space cooling","A Condition (35°C - 27/19)","","EERd","","1.88"]
["","","","Pdc","kW","28.0"]
["","B Condition (30°C - 27/19)","","EERd","","2.88"]
["","","","Pdc","kW","20.6"]
["","C Condition (25°C - 27/19)","","EERd","","6.40"]
["","","","Pdc","kW","13.3"]
["","D Condition (20°C - 27/19)","","EERd","","12.3"]
["","","","Pdc","kW","8.28"]
["Space cooling recommended combination 2","A Condition (35°C - 27/19)","","EERd","","1.88"]
["","","","Pdc","kW","28.0"]
["","B Condition (30°C - 27/19)","","EERd","","2.88"]
["","","","Pdc","kW","20.6"]
["","C Condition (25°C - 27/19)","","EERd","","6.40"]
["","","","Pdc","kW","13.3"]
["","D Condition (20°C - 27/19)","","EERd","","12.3"]
["","","","Pdc","kW","8.28"]
["Space heating (Average climate)","TBivalent","","COPd (declared COP)","","1.53"]
["","","","Pdh (declared heating cap)","kW","16.0"]
["","","","Tbiv (bivalent temperature)","°C","-10.0"]
["","Space heating (Average climate)-=-E condition (-10°C)","","Space heating (Average climate)-=-E condition (-10°C)-=-COPd (declared COP)","","1.53"]
["","","","Space heating (Average climate)-=-E condition (-10°C)-=-Pdh (declared heating cap)-=-kW","kW","16.0"]
["","TOL","","Tol (temperature operating limit)","°C","-10"]
["","A Condition (-7°C)","","COPd (declared COP)","","2.14"]
["","","","Pdh (declared heating cap)","kW","14.2"]
["","B Condition (2°C)","","COPd (declared COP)","","3.34"]
["","","","Pdh (declared heating cap)","kW","8.62"]
["","C Condition (7°C)","","COPd (declared COP)","","5.00"]
["","","","Pdh (declared heating cap)","kW","5.54"]
["","D Condition (12°C)","","COPd (declared COP)","","6.52"]
["","","","Pdh (declared heating cap)","kW","7.04"]
["Space heating (Average climate) recommended combination 2","TBivalent","","COPd (declared COP)","","1.53"]
["","","","Pdh (declared heating cap)","kW","16.0"]
["","","","Tbiv (bivalent temperature)","°C","-10.0"]
["","TOL","","COPd (declared COP)","","1.53"]
["","","","Pdh (declared heating cap)","kW","16.0"]
["","","","Tol (temperature operating limit)","°C","-10"]
["","A Condition (-7°C)","","COPd (declared COP)","","2.14"]
["","","","Pdh (declared heating cap)","kW","14.2"]
["","B Condition (2°C)","","COPd (declared COP)","","3.34"]
["","","","Pdh (declared heating cap)","kW","8.62"]
["","C Condition (7°C)","","COPd (declared COP)","","5.00"]
["","","","Pdh (declared heating cap)","kW","5.54"]
["","D Condition (12°C)","","COPd (declared COP)","","6.52"]
["","","","Pdh (declared heating cap)","kW","7.04"]
["Capacity range","HP","","","","10"]
["Maximum number of connectable indoor units","","","","","8 (3)"]
["Indoor index connection","Min.","","","","125"]
["","Max.","","","","325"]
["Dimensions","Unit","","Height","mm","1,680"]
["","","","Width","mm","1930"]
["","","","Depth","mm","765"]
["Weight","Unit","","","kg","564"]
["Compressor","Type","","","","Hermetically sealed swing compressor"]
["Operation range","Cooling","","Min.","°CDB","-5"]
["","","","Max.","°CDB","43"]
["","Heating","","Min.","°CWB","-20"]
["","","","Max.","°CWB","16"]
["Sound power level","Cooling","","Nom.","dBA","835.0 (4)"]
["Sound pressure level","Cooling","","Nom.","dBA","608.0 (5)"]
["Refrigerant","Type","","","","R744 (CO2)"]
["","GWP","","","","1.0"]
["","Charge","","","tCO2Eq","0.00"]
["","Charge","","","kg","0.00"]
["Piping connections","Liquid","","Type","","Braze connection"]
["","","","OD","mm","9.52"]
["","Gas","","Type","","Braze connection"]
["","","","OD","mm","15.9"]
["","Total piping length","System","Actual","m","300 (6)"]
["Standard Accessories","Installation manual","","","","1"]
["","Auxiliary piping set","","","","1"]
["","General safety precautions","","","","1"]
["","Operation manual","","","","1"]
["","Safety valve","","","","2"]
["","Changeover valve","","","","1"]
["","Declaration of conformity","","","","1"]
["Power supply","Name","","","","Y1"]
["","Phase","","","","3N~"]
["","Frequency","","","Hz","50"]
["","Voltage","","","V","380-415"]
["Notes","","","","","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 7.5m; level difference: 0m"]
["","","","","","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 7.5m; level difference: 0m"]
["","","","","","(3) - The actual number of units depends on the connection ratio (CR) and the restrictions for the system."]
["","","","","","(4) - Sound power level is an absolute value that a sound source generates."]
["","","","","","(5) - Sound pressure level is a relative value, depending on the distance and acoustic environment. For more details, please refer to the sound level drawings."]
["","","","","","(6) - Refer to refrigerant pipe selection or installation manual"]
["","","","","","(7) - RLA is based on following conditions: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB"]
["","","","","","(8) - MSC means the maximum current during start up of the compressor. This unit uses only inverter compressors. Starting current is always ≤ max. running current."]
["","","","","","(9) - In accordance with EN/IEC 61000-3-12, it may be necessary to consult the distribution network operator to ensure that the equipment is connected only to a supply wih Ssc  ≥ minimum Ssc value"]
["","","","","","(10) - MCA must be used to select the correct field wiring size. The MCA can be regarded as the maximum running current."]
["","","","","","(11) - MFA is used to select the circuit breaker and the ground fault circuit interrupter (earth leakage circuit breaker)."]
["","","","","","(12) - Maximum allowable voltage range variation between phases is 2%."]
["","","","","","(13) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits."]
["","","","","","(14) - Sound values are measured in a semi-anechoic room."]
["","","","","","(15) - EN/IEC 61000-3-12: European/international technical standard setting the limits for harmonic currents produced by equipment connected to public low-voltage system with input current > 16A and ≤ 75A per phase"]
["","","","","","(16) - Ssc: Short-circuit power"]
["","","","","","(17) - For detailed contents of standard accessories, see installation/operation manual"]