{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":9,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZAG-LV1"]
[]
[]
[]
[]
["","","","","","RZAG71L7V1B","RZAG100L7V1B","RZAG125L7V1B","RZAG140L7V1B"]
["Sound pressure level","Heating","","Nom.","dBA","50","51","52","52"]
["","Cooling","","Nom.","dBA","48","49","51","52"]
["","Night quiet mode","","Level 1","dBA","43","45","45","45"]
["Standard Accessories","Tie-wraps","","","","2","2","2","2"]
["","Installation manual","","","","1","1","1","1"]
["Refrigerant","Charge","","","TCO2Eq","1.8","2.3","2.3","2.3"]
["","GWP","","","","675","675","675","675"]
["","Charge","","","kg","2.6","3.4","3.4","3.4"]
["","Type","","","","R-32","R-32","R-32","R-32"]
["Piping connections","Liquid","","OD","mm","9.52","9.52","9.52","9.52"]
["","Piping length","OU - IU","Max.","m","55","85","85","85"]
["","","System","Chargeless","m","30","30","30","30"]
["","","","Equivalent","m","75","100","100","100"]
["","Gas","","OD","mm","15.9","15.9","15.9","15.9"]
["","Level difference","IU - IU","Max.","m","0.5","0.5","0.5","0.5"]
["","","IU - OU","Max.","m","30.0","30.0","30.0","30.0"]
["","Additional refrigerant charge","","","kg/m","See installation manual","See installation manual","See installation manual","See installation manual"]
["Sound power level","Cooling","","","dBA","64","64","66","67"]
["Dimensions","Unit","","Width","mm","940","940","940","940"]
["","","","Depth","mm","320","320","320","320"]
["","","","Height","mm","990","1,430","1,430","1,430"]
["Compressor","Type","","","","Hermetically sealed swing compressor","Hermetically sealed swing compressor","Hermetically sealed swing compressor","Hermetically sealed swing compressor"]
["Weight","Unit","","","kg","67","93","93","93"]
["Power supply","Phase","","","","1~","1~","1~","1~"]
["","Frequency","","","Hz","50/60","50/60","50/60","50/60"]
["","Voltage","","","V","220-240","220-240","220-240","220-240"]
["Notes","","","","","(1) - Contains fluorinated greenhouse gases","(1) - Contains fluorinated greenhouse gases","(1) - Contains fluorinated greenhouse gases","(1) - Contains fluorinated greenhouse gases"]
["","","","","","(2) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m. Data for standard efficiency series","(2) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m. Data for standard efficiency series","(2) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m. Data for standard efficiency series","(2) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m. Data for standard efficiency series"]
["","","","","","(3) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m. Data for standard efficiency series","(3) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m. Data for standard efficiency series","(3) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m. Data for standard efficiency series","(3) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m. Data for standard efficiency series"]
["","","","","","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data"]