{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":82,"n_cols":21,"rows_kept":82,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","UATYA-BFC2Y1"]
[]
[]
[]
[]
["","","","","","UATYA25BFC2Y1","UATYA30BFC2Y1","UATYA40BFC2Y1","UATYA50BFC2Y1","UATYA60BFC2Y1","UATYA70BFC2Y1","UATYA80BFC2Y1","UATYA90BFC2Y1","UATYA100BFC2Y1","UATYA110BFC2Y1","UATYA120BFC2Y1","UATYA140BFC2Y1","UATYA150BFC2Y1","UATYA160BFC2Y1","UATYA180BFC2Y1","UATYA190BFC2Y1"]
["Cooling capacity","Nom.","","","kW","","","","","58.8 (1)","65.3 (1)"]
["","With 30% fresh air","","","kW","","","","","63.0 (1)","69.9 (1)"]
["Heating capacity","Nom.","","","kW","","","","","55.1 (2)","64.9 (2)"]
["","With 30% fresh air","","","kW","","","","","55.1 (2)","65.1 (2)"]
["Power input","Cooling","","Nom.","kW","","","","","18.8 (1)","22.4 (1)"]
["","Heating","","Nom.","kW","","","","","16.9 (2)","20.2 (2)"]
["EER","","","","","2.83 (1), 2.96 (3)","3.09 (1), 3.26 (3)","3.06 (1), 3.21 (3)","2.96 (1), 3.10 (3)","3.12 (1), 3.28 (3)","2.92 (1), 3.06 (3)","3.09 (1), 3.26 (3)","3.06 (1), 3.24 (3)","2.97 (1), 3.13 (3)","2.99 (1), 3.13 (3)","2.91 (1), 3.03 (3)","3.14 (1), 3.29 (3)","3.02 (1), 3.16 (3)","3.05 (1), 3.19 (3)","3.07 (1), 3.21 (3)","2.97 (1), 3.10 (3)"]
["COP","","","","","3.22 (2), 3.43 (3)","3.31 (2), 3.53 (3)","3.26 (2), 3.48 (3)","3.24 (2), 3.51 (3)","3.25 (2), 3.47 (3)","3.21 (2), 3.44 (3)","3.37 (2), 3.62 (3)","3.22 (2), 3.47 (3)","3.20 (2), 3.46 (3)","3.35 (2), 3.60 (3)","3.25 (2), 3.48 (3)","3.44 (2), 3.69 (3)","3.33 (2), 3.57 (3)","3.26 (2), 3.50 (3)","3.33 (2), 3.58 (3)","3.27 (2), 3.55 (3)"]
["Space cooling","Capacity","","Pdesign","kW","","","","","58.8","65.3"]
["","SEER","","","","","","","","5.50 (4)","4.53 (4)"]
["Space heating (Average climate)","Capacity","","Pdesign","kW","","","","","55.1","64.9"]
["","SCOP/A","","","","","","","","3.47 (4)","3.41 (4)"]
["Evaporator","Supply side","Fan","Air flow rate","m³/h","","","","","11,000","13,000"]
["","","","High ESP","Pa","","","","","629 (5)","410 (5)"]
["","","","Nominal ESP","Pa","","","","","300 (5)","300 (5)"]
["","Fresh air","Ratio","Standard","%","","","","","30","30"]
["","","","In free cooling","%","","","","","100","100"]
["Operation range","Cooling","","Min.","°CDB","","","","","-10","-10"]
["","","","Max.","°CDB","","","","","48","48"]
["","Heating","","Min.","°CWB","","","","","-15","-15"]
["","","","Max.","°CWB","","","","","26","26"]
["Condenser","Air flow rate","","Cooling","m³/h","","","","","31,183","32,203"]
["","Refrigerant","","GWP","","","","","","675","675"]
["","","","Charge","kg","","","","","18.0","18.0"]
["Dimensions","Unit","","Height","mm","","","","","1,924","1,924"]
["","","","Width","mm","","","","","2,250","2,250"]
["","","","Depth","mm","","","","","4,879","4,879"]
["Weight","Unit","","","kg","","","","","1,703","1,803"]
["Sound pressure level","Cooling","","","dBA","","","","","69.0 (6)","68.1 (6)"]
["Sound power level","Cooling","","","dBA","","","","","88.5 (7)","87.5 (7)"]
["Power supply","Name","","","","","","","","400/3/50±5%","400/3/50±5%"]
["","Phase","","","","","","","","3~","3~"]
["","Frequency","","","Hz","","","","","50","50"]
["","Voltage","","","V","","","","","400","400"]
["Current","Recommended fuses","","","A","","","","","50","63"]
["Notes","","","","","(1) - Conditions for calculation: Ambient air 27°C DB, 19°C WB; External air 35°C DB, 24°C WB. 100% recirculating air; calculated according to EN 14511/2018","(1) - Conditions for calculation: Ambient air 27°C DB, 19°C WB; External air 35°C DB, 24°C WB. 100% recirculating air; calculated according to EN 14511/2018","(1) - Conditions for calculation: Ambient air 27°C DB, 19°C WB; External air 35°C DB, 24°C WB. 100% recirculating air; calculated according to EN 14511/2018","(1) - Conditions for calculation: Ambient air 27°C DB, 19°C WB; External air 35°C DB, 24°C WB. 100% recirculating air; calculated according to EN 14511/2018","(1) - Conditions for calculation: Ambient air 27°C DB, 19°C WB; External air 35°C DB, 24°C WB. 100% recirculating air; calculated according to EN 14511/2018","(1) - Conditions for calculation: Ambient air 27°C DB, 19°C WB; External air 35°C DB, 24°C WB. 100% recirculating air; calculated according to EN 14511/2018","(1) - Conditions for calculation: Ambient air 27°C DB, 19°C WB; External air 35°C DB, 24°C WB. 100% recirculating air; calculated according to EN 14511/2018","(1) - Conditions for calculation: Ambient air 27°C DB, 19°C WB; External air 35°C DB, 24°C WB. 100% recirculating air; calculated according to EN 14511/2018","(1) - Conditions for calculation: Ambient air 27°C DB, 19°C WB; External air 35°C DB, 24°C WB. 100% recirculating air; calculated according to EN 14511/2018","(1) - Conditions for calculation: Ambient air 27°C DB, 19°C WB; External air 35°C DB, 24°C WB. 100% recirculating air; calculated according to EN 14511/2018","(1) - Conditions for calculation: Ambient air 27°C DB, 19°C WB; External air 35°C DB, 24°C WB. 100% recirculating air; calculated according to EN 14511/2018","(1) - Conditions for calculation: Ambient air 27°C DB, 19°C WB; External air 35°C DB, 24°C WB. 100% recirculating air; calculated according to EN 14511/2018","(1) - Conditions for calculation: Ambient air 27°C DB, 19°C WB; External air 35°C DB, 24°C WB. 100% recirculating air; calculated according to EN 14511/2018","(1) - Conditions for calculation: Ambient air 27°C DB, 19°C WB; External air 35°C DB, 24°C WB. 100% recirculating air; calculated according to EN 14511/2018","(1) - Conditions for calculation: Ambient air 27°C DB, 19°C WB; External air 35°C DB, 24°C WB. 100% recirculating air; calculated according to EN 14511/2018","(1) - Conditions for calculation: Ambient air 27°C DB, 19°C WB; External air 35°C DB, 24°C WB. 100% recirculating air; calculated according to EN 14511/2018"]
["","","","","","(2) - Conditions for calculation: Ambient air 20°C DB, 15°C WB; External air 7°C DB, 6°C WB. 100% recirculating air; calculated according to EN 14511/2018","(2) - Conditions for calculation: Ambient air 20°C DB, 15°C WB; External air 7°C DB, 6°C WB. 100% recirculating air; calculated according to EN 14511/2018","(2) - Conditions for calculation: Ambient air 20°C DB, 15°C WB; External air 7°C DB, 6°C WB. 100% recirculating air; calculated according to EN 14511/2018","(2) - Conditions for calculation: Ambient air 20°C DB, 15°C WB; External air 7°C DB, 6°C WB. 100% recirculating air; calculated according to EN 14511/2018","(2) - Conditions for calculation: Ambient air 20°C DB, 15°C WB; External air 7°C DB, 6°C WB. 100% recirculating air; calculated according to EN 14511/2018","(2) - Conditions for calculation: Ambient air 20°C DB, 15°C WB; External air 7°C DB, 6°C WB. 100% recirculating air; calculated according to EN 14511/2018","(2) - Conditions for calculation: Ambient air 20°C DB, 15°C WB; External air 7°C DB, 6°C WB. 100% recirculating air; calculated according to EN 14511/2018","(2) - Conditions for calculation: Ambient air 20°C DB, 15°C WB; External air 7°C DB, 6°C WB. 100% recirculating air; calculated according to EN 14511/2018","(2) - Conditions for calculation: Ambient air 20°C DB, 15°C WB; External air 7°C DB, 6°C WB. 100% recirculating air; calculated according to EN 14511/2018","(2) - Conditions for calculation: Ambient air 20°C DB, 15°C WB; External air 7°C DB, 6°C WB. 100% recirculating air; calculated according to EN 14511/2018","(2) - Conditions for calculation: Ambient air 20°C DB, 15°C WB; External air 7°C DB, 6°C WB. 100% recirculating air; calculated according to EN 14511/2018","(2) - Conditions for calculation: Ambient air 20°C DB, 15°C WB; External air 7°C DB, 6°C WB. 100% recirculating air; calculated according to EN 14511/2018","(2) - Conditions for calculation: Ambient air 20°C DB, 15°C WB; External air 7°C DB, 6°C WB. 100% recirculating air; calculated according to EN 14511/2018","(2) - Conditions for calculation: Ambient air 20°C DB, 15°C WB; External air 7°C DB, 6°C WB. 100% recirculating air; calculated according to EN 14511/2018","(2) - Conditions for calculation: Ambient air 20°C DB, 15°C WB; External air 7°C DB, 6°C WB. 100% recirculating air; calculated according to EN 14511/2018","(2) - Conditions for calculation: Ambient air 20°C DB, 15°C WB; External air 7°C DB, 6°C WB. 100% recirculating air; calculated according to EN 14511/2018"]
["","","","","","(3) - With 30% fresh air","(3) - With 30% fresh air","(3) - With 30% fresh air","(3) - With 30% fresh air","(3) - With 30% fresh air","(3) - With 30% fresh air","(3) - With 30% fresh air","(3) - With 30% fresh air","(3) - With 30% fresh air","(3) - With 30% fresh air","(3) - With 30% fresh air","(3) - With 30% fresh air","(3) - With 30% fresh air","(3) - With 30% fresh air","(3) - With 30% fresh air","(3) - With 30% fresh air"]
["","","","","","(4) - Calculated according to EN 14825/2019","(4) - Calculated according to EN 14825/2019","(4) - Calculated according to EN 14825/2019","(4) - Calculated according to EN 14825/2019","(4) - Calculated according to EN 14825/2019","(4) - Calculated according to EN 14825/2019","(4) - Calculated according to EN 14825/2019","(4) - Calculated according to EN 14825/2019","(4) - Calculated according to EN 14825/2019","(4) - Calculated according to EN 14825/2019","(4) - Calculated according to EN 14825/2019","(4) - Calculated according to EN 14825/2019","(4) - Calculated according to EN 14825/2019","(4) - Calculated according to EN 14825/2019","(4) - Calculated according to EN 14825/2019","(4) - Calculated according to EN 14825/2019"]
["","","","","","(5) - Value refers to unit at nominal airflow, delivered with no accessories and with only G4 filters.","(5) - Value refers to unit at nominal airflow, delivered with no accessories and with only G4 filters.","(5) - Value refers to unit at nominal airflow, delivered with no accessories and with only G4 filters.","(5) - Value refers to unit at nominal airflow, delivered with no accessories and with only G4 filters.","(5) - Value refers to unit at nominal airflow, delivered with no accessories and with only G4 filters.","(5) - Value refers to unit at nominal airflow, delivered with no accessories and with only G4 filters.","(5) - Value refers to unit at nominal airflow, delivered with no accessories and with only G4 filters.","(5) - Value refers to unit at nominal airflow, delivered with no accessories and with only G4 filters.","(5) - Value refers to unit at nominal airflow, delivered with no accessories and with only G4 filters.","(5) - Value refers to unit at nominal airflow, delivered with no accessories and with only G4 filters.","(5) - Value refers to unit at nominal airflow, delivered with no accessories and with only G4 filters.","(5) - Value refers to unit at nominal airflow, delivered with no accessories and with only G4 filters.","(5) - Value refers to unit at nominal airflow, delivered with no accessories and with only G4 filters.","(5) - Value refers to unit at nominal airflow, delivered with no accessories and with only G4 filters.","(5) - Value refers to unit at nominal airflow, delivered with no accessories and with only G4 filters.","(5) - Value refers to unit at nominal airflow, delivered with no accessories and with only G4 filters."]
["","","","","","(6) - Average sound pressure level, at 1 meter from the unit, in  free field on a reflective surface. Not binding value derived from the sound power level","(6) - Average sound pressure level, at 1 meter from the unit, in  free field on a reflective surface. Not binding value derived from the sound power level","(6) - Average sound pressure level, at 1 meter from the unit, in  free field on a reflective surface. Not binding value derived from the sound power level","(6) - Average sound pressure level, at 1 meter from the unit, in  free field on a reflective surface. Not binding value derived from the sound power level","(6) - Average sound pressure level, at 1 meter from the unit, in  free field on a reflective surface. Not binding value derived from the sound power level","(6) - Average sound pressure level, at 1 meter from the unit, in  free field on a reflective surface. Not binding value derived from the sound power level","(6) - Average sound pressure level, at 1 meter from the unit, in  free field on a reflective surface. Not binding value derived from the sound power level","(6) - Average sound pressure level, at 1 meter from the unit, in  free field on a reflective surface. Not binding value derived from the sound power level","(6) - Average sound pressure level, at 1 meter from the unit, in  free field on a reflective surface. Not binding value derived from the sound power level","(6) - Average sound pressure level, at 1 meter from the unit, in  free field on a reflective surface. Not binding value derived from the sound power level","(6) - Average sound pressure level, at 1 meter from the unit, in  free field on a reflective surface. Not binding value derived from the sound power level","(6) - Average sound pressure level, at 1 meter from the unit, in  free field on a reflective surface. Not binding value derived from the sound power level","(6) - Average sound pressure level, at 1 meter from the unit, in  free field on a reflective surface. Not binding value derived from the sound power level","(6) - Average sound pressure level, at 1 meter from the unit, in  free field on a reflective surface. Not binding value derived from the sound power level","(6) - Average sound pressure level, at 1 meter from the unit, in  free field on a reflective surface. Not binding value derived from the sound power level","(6) - Average sound pressure level, at 1 meter from the unit, in  free field on a reflective surface. Not binding value derived from the sound power level"]
["","","","","","(7) - Sound power level in free field calculated according to standard ISO  3744. Values refer only to the base unit version","(7) - Sound power level in free field calculated according to standard ISO  3744. Values refer only to the base unit version","(7) - Sound power level in free field calculated according to standard ISO  3744. Values refer only to the base unit version","(7) - Sound power level in free field calculated according to standard ISO  3744. Values refer only to the base unit version","(7) - Sound power level in free field calculated according to standard ISO  3744. Values refer only to the base unit version","(7) - Sound power level in free field calculated according to standard ISO  3744. Values refer only to the base unit version","(7) - Sound power level in free field calculated according to standard ISO  3744. Values refer only to the base unit version","(7) - Sound power level in free field calculated according to standard ISO  3744. Values refer only to the base unit version","(7) - Sound power level in free field calculated according to standard ISO  3744. Values refer only to the base unit version","(7) - Sound power level in free field calculated according to standard ISO  3744. Values refer only to the base unit version","(7) - Sound power level in free field calculated according to standard ISO  3744. Values refer only to the base unit version","(7) - Sound power level in free field calculated according to standard ISO  3744. Values refer only to the base unit version","(7) - Sound power level in free field calculated according to standard ISO  3744. Values refer only to the base unit version","(7) - Sound power level in free field calculated according to standard ISO  3744. Values refer only to the base unit version","(7) - Sound power level in free field calculated according to standard ISO  3744. Values refer only to the base unit version","(7) - Sound power level in free field calculated according to standard ISO  3744. Values refer only to the base unit version"]
["Operation range","Heating","","Max.","°CWB","26","26","26","26","","","26","26","26","26","26","26","26","26","26","26"]
["","","","Min.","°CWB","-15","-15","-15","-15","","","-15","-15","-15","-15","-15","-15","-15","-15","-15","-15"]
["","Cooling","","Max.","°CDB","48","48","48","48","","","48","48","48","48","48","48","48","48","48","48"]
["","","","Min.","°CDB","-10","-10","-10","-10","","","-10","-10","-10","-10","-10","-10","-10","-10","-10","-10"]
["Cooling capacity","Nom.","","","kW","24.1 (1)","31.3 (1)","38.7 (1)","45.7 (1)","","","74.8 (1)","89.8 (1)","95.8 (1)","108.9 (1)","115.0 (1)","133.4 (1)","144.7 (1)","154.6 (1)","171.9 (1)","187.0 (1)"]
["","With 30% fresh air","","","kW","25.8 (1)","33.6 (1)","41.5 (1)","48.9 (1)","","","80.7 (1)","96.6 (1)","102.7 (1)","117.0 (1)","122.7 (1)","143.1 (1)","154.9 (1)","165.7 (1)","184.2 (1)","200.5 (1)"]
["Heating capacity","Nom.","","","kW","24.0 (2)","29.5 (2)","36.3 (2)","46.2 (2)","","","68.5 (2)","84.2 (2)","92.8 (2)","101.5 (2)","108.0 (2)","123.1 (2)","136.4 (2)","147.1 (2)","157.1 (2)","176.9 (2)"]
["","With 30% fresh air","","","kW","24.3 (2)","29.6 (2)","36.5 (2)","46.3 (2)","","","69.2 (2)","84.7 (2)","94.8 (2)","102.1 (2)","108.7 (2)","124.2 (2)","137.5 (2)","148.4 (2)","158.7 (2)","180.2 (2)"]
["Power input","Cooling","","Nom.","kW","8.5 (1)","10.1 (1)","12.7 (1)","15.4 (1)","","","24.2 (1)","29.4 (1)","32.3 (1)","36.4 (1)","39.5 (1)","42.5 (1)","47.9 (1)","50.7 (1)","56.1 (1)","62.9 (1)"]
["","Heating","","Nom.","kW","7.5 (2)","8.9 (2)","11.1 (2)","14.2 (2)","","","20.3 (2)","26.1 (2)","29.0 (2)","30.3 (2)","33.2 (2)","35.8 (2)","40.9 (2)","45.1 (2)","47.2 (2)","54.2 (2)"]
["Space cooling","Capacity","","Pdesign","kW","24.1","31.3","38.7","45.7","","","74.8","89.8","95.8","108.9","115.0","133.4","144.7","154.6","171.9","187.0"]
["","SEER","","","","4.52 (4)","4.79 (4)","5.39 (4)","5.26 (4)","","","5.56 (4)","5.47 (4)","5.17 (4)","5.29 (4)","5.15 (4)","4.38 (4)","4.26 (4)","4.27 (4)","4.15 (4)","4.08 (4)"]
["Space heating (Average climate)","Capacity","","Pdesign","kW","24.0","29.5","36.3","46.2","","","68.5","84.2","92.8","101.5","108.0","123.1","136.4","147.1","157.1","176.9"]
["","SCOP/A","","","","3.35 (4)","3.38 (4)","3.67 (4)","3.65 (4)","","","3.70 (4)","3.65 (4)","3.62 (4)","3.56 (4)","3.53 (4)","3.39 (4)","3.36 (4)","3.34 (4)","3.31 (4)","3.34 (4)"]
["Evaporator","Supply side","Fan","Air flow rate","m³/h","4500","5800","7500","9000","","","14500","16500","18000","19800","21600","25000","26500","28000","30500","31500"]
["","","","Nominal ESP","Pa","300 (5)","300 (5)","300 (5)","300 (5)","","","300 (5)","300 (5)","300 (5)","300 (5)","300 (5)","300 (5)","300 (5)","300 (5)","300 (5)","300 (5)"]
["","","","High ESP","Pa","425 (5)","727 (5)","510 (5)","439 (5)","","","526 (5)","493 (5)","463 (5)","427 (5)","394 (5)","441 (5)","416 (5)","388 (5)","340 (5)","310 (5)"]
["","Fresh air","Ratio","Standard","%","30","30","30","30","","","30","30","30","30","30","30","30","30","30","30"]
["","","","In free cooling","%","100","100","100","100","","","100","100","100","100","100","100","100","100","100","100"]
["Condenser","Air flow rate","","Cooling","m³/h","15725","16038","16374","16341","","","35774","37285","36195","38143","36865","70704","72395","67733","70200","72005"]
["","Refrigerant","","GWP","","675","675","675","675","","","675","675","675","675","675","675","675","675","675","675"]
["","","","Charge","tCO2Eq","4725","6750","8100","10125","","","15525","16200","18900","20250","24300","25650","25650","31050","33750","33750"]
["","","","Charge","kg","7.0","10.0","12.0","15.0","","","23.0","24.0","28.0","30.0","36.0","38.0","38.0","46.0","50.0","50.0"]
["Dimensions","Unit","","Height","mm","1924","1924","2374","2374","","","2374","2374","2374","2374","2374","2374","2374","2374","2374","2374"]
["","","","Width","mm","2250","2250","2250","2250","","","2250","2250","2250","2250","2250","2250","2250","2250","2250","2250"]
["","","","Depth","mm","2943","2943","2943","2943","","","4879","4879","4879","4879","4879","5679","5679","5679","5679","5679"]
["Weight","Unit","","","kg","981","1014","1084","1143","","","1984","2040","2110","2196","2206","2658","2668","2708","2746","2828"]
["Sound pressure level","Cooling","","","dBA","63.9 (6)","66.0 (6)","68.0 (6)","67.3 (6)","","","72.6 (6)","68.7 (6)","69.9 (6)","70.6 (6)","74.2 (6)","68.3 (6)","68.3 (6)","68.7 (6)","69.1 (6)","70.0 (6)"]
["Sound power level","Cooling","","","dBA","82.2 (7)","84.3 (7)","86.8 (7)","86.1 (7)","","","92.5 (7)","88.6 (7)","89.8 (7)","90.5 (7)","94.1 (7)","88.6 (7)","88.6 (7)","89.0 (7)","89.3 (7)","90.2 (7)"]
["Power supply","Name","","","","400/3/50±5%","400/3/50±5%","400/3/50±5%","400/3/50±5%","","","400/3/50±5%","400/3/50±5%","400/3/50±5%","400/3/50±5%","400/3/50±5%","400/3/50±5%","400/3/50±5%","400/3/50±5%","400/3/50±5%","400/3/50±5%"]
["","Phase","","","","3~","3~","3~","3~","","","3~","3~","3~","3~","3~","3~","3~","3~","3~","3~"]
["","Frequency","","","Hz","50","50","50","50","","","50","50","50","50","50","50","50","50","50","50"]
["","Voltage","","","V","400","400","400","400","","","400","400","400","400","400","400","400","400","400","400"]
["Current","Recommended fuses","","","A","25","40","40","50","","","80","100","100","100","100","160","160","160","200","200"]