{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":6,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","UK.MC55W"]
[]
[]
[]
[]
["","","","","","UK.MC55W."]
["Sound pressure level","Air purifying operation","","Turbo","dBA","53"]
["","","","Medium","dBA","39"]
["","","","Low","dBA","29"]
["","","","Silent","dBA","19"]
["Standard Accessories","Remote controller","","","","1"]
["","Remote control holder","","","","1"]
["","Electrostatic HEPA filter","","","","1"]
["","Deodorising filter","","","","1"]
["","Operation manual","","","","1"]
["Safety devices","Item","","01","","Safety switch (Operation stops when the Streamer unit cover is open)"]
["Dimensions","Unit","","Width","mm","270"]
["","","","Depth","mm","270"]
["","","","Height","mm","500"]
["Casing","Colour","","","","White"]
["Applicable room area","m²","","","","41 (1), 82 (2)"]
["Dust collecting method","","","","","Electrostatic HEPA filter"]
["Deodorizing method","","","","","Flash streamer + Deodorizing catalyst"]
["Weight","Unit","","","kg","6.8"]
["Type","","","","","Air Purifier"]
["Fan","Air flow rate","Air purifying operation","Turbo","m³/h","330"]
["","","","Silent","m³/h","66"]
["","","","Low","m³/h","120"]
["","","","Medium","m³/h","192"]
["CADR","m³/h","","","","320"]
["Application","","","","","Floor standing type"]
["Air purifying operation","Power input","","Turbo","kW","0.037"]
["","","","Silent","kW","0.008"]
["","","","L","kW","0.010"]
["","","","M","kW","0.015"]
["Running current","Air purifying operation","","Low","A","0.10"]
["","","","Turbo","A","0.32"]
["","","","Medium","A","0.14"]
["","","","Silent","A","0.08"]
["Power supply","Phase","","","","1~"]
["","Frequency","","","Hz","50/60"]
["","Voltage","","","V","220-240/220-230"]
["Notes","","","","","(1) - The applicable room area is appropriate for operating the unit of maximum fan speed (HH). Applicable room area indicates  the space where a certain amount of dust particles can be remover in 30 minutes. (JEM 1467)"]
["","","","","","(2) - Converted to NRCC standards from test values in accordance with JEM1467."]
["","","","","","(3) - Converted to CADR standards from test values in accordance with JEM1467."]
["","","","","","(4) - Operating sound levels are the average of values measured at 1m away from the front, left, right and top of the unit. (These are equal to the values in an anechoic chamber)"]
["","","","","","(5) - Electrostatic HEPA filter is attached in the unit."]
["","","","","","(6) - Other function: Active plasmation function. Auto-restart function."]
["Power cord","m","","","","1.8"]