{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":68,"n_cols":6,"rows_kept":68,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","UK.MCK55W"]
[]
[]
[]
[]
["","","","","","UK.MCK55W."]
["Sound pressure level","Air purifying operation","","Turbo","dBA","53.0"]
["","","","Medium","dBA","39.0"]
["","","","Low","dBA","29.0"]
["","","","Silent","dBA","19.0"]
["","Humidifying operation","","Medium","dBA","39.0"]
["","","","Turbo","dBA","53.0"]
["","","","Low","dBA","33.0"]
["","","","Silent","dBA","25.0"]
["Standard Accessories","Remote control lid","","","","1"]
["","Remote control holder","","","","1"]
["","Electrostatic HEPA filter","","","","1"]
["","Humidifying filter","","","","2"]
["","Deodorising filter","","","","1"]
["","Operation manual","","","","1"]
["","Caster","","","","4"]
["Humidifying operation","Power input","","L","kW","0.014"]
["","","","Silent","kW","0.011"]
["","","","M","kW","0.019"]
["","","","Turbo","kW","0.058"]
["","Water tank capacity","","","l","2.7"]
["Dimensions","Unit","","Width","mm","270"]
["","","","Depth","mm","270"]
["","","","Height","mm","700"]
["Casing","Colour","","","","White"]
["Applicable room area","m²","","","","41 (1), 82 (2)"]
["Dust collecting method","","","","","Electrostatic HEPA filter"]
["Deodorizing method","","","","","Flash streamer + Deodorizing catalyst"]
["Weight","Unit","","","kg","9.5"]
["Type","","","","","Humidifying air purifier"]
["Fan","Air flow rate","Air purifying operation","Turbo","m³/h","330"]
["","","","Silent","m³/h","54"]
["","","","Low","m³/h","120"]
["","","","Medium","m³/h","192"]
["","","Humidifying operation","Low","m³/h","144"]
["","","","Silent","m³/h","102"]
["","","","Medium","m³/h","192"]
["","","","Turbo","m³/h","330"]
["CADR","m³/h","","","","320"]
["Application","","","","","Floor standing type"]
["Air purifying operation","Power input","","Turbo","kW","0.056"]
["","","","Silent","kW","0.007"]
["","","","L","kW","0.010"]
["","","","M","kW","0.017"]
["Running current","Air purifying operation","","Low","A","0.12"]
["","","","Turbo","A","0.50"]
["","","","Medium","A","0.19"]
["","","","Silent","A","0.09"]
["","Humidifying operation","","Silent","A","0.13"]
["","","","Low","A","0.15"]
["","","","Turbo","A","0.50"]
["","","","Medium","A","0.20"]
["Power supply","Phase","","","","1~"]
["","Frequency","","","Hz","50/60"]
["","Voltage","","","V","220-240/220-230"]
["Notes","","","","","(1) - The applicable room area is appropriate for operating the unit of maximum fan speed (HH). Applicable room area indicates  the space where a certain amount of dust particles can be remover in 30 minutes. (JEM 1467)"]
["","","","","","(2) - Converted to NRCC standards from test values in accordance with JEM1467."]
["","","","","","(3) - Converted to CADR standards from test values in accordance with JEM1467."]
["","","","","","(4) - Humidification amount changes in accordance with indoor and outdoor temperature and humidity. Measurement condition: 20°C in temperature, 30% in humidity."]
["","","","","","(5) - Operating sound levels are the average of values measured at 1m away from the front, left, right and top of the unit. (These are equal to the values in an anechoic chamber)"]
["","","","","","(6) - Electrostatic HEPA filter and humidifying filters are attached in the unit."]
["","","","","","(7) - Requirements according to JEM1467."]
["Power cord","m","","","","1.8"]