{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":40,"n_cols":7,"rows_kept":40,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","VAM-FC9"]
[]
[]
[]
[]
["","","","","","VAM150FCVE9","VAM250FCVE9"]
["Power input - 50Hz","Heat exchange mode","Nom.","Ultra high","kW","0.132","0.161"]
["","Bypass mode","Nom.","Ultra high","kW","0.132","0.161"]
["Casing","Material","","","","Galvanised steel plate","Galvanised steel plate"]
["Dimensions","Unit","","Height","mm","285","285"]
["","","","Width","mm","776","776"]
["","","","Depth","mm","525","525"]
["Weight","Unit","","","kg","23","23"]
["Fan","Air flow rate - 50Hz","Heat exchange mode","Ultra high","m³/h","150","250"]
["","","Bypass mode","Ultra high","m³/h","150","250"]
["","External static pressure - 50Hz","","Ultra high","Pa","90.0","70.0"]
["Operation range","Min.","","","°CDB","-15","-15"]
["","Max.","","","°CDB","50","50"]
["","Relative humidity","","","%","80 or less","80 or less"]
["Sound pressure level - 50Hz","Heat exchange mode","","Ultra high","dBA","27.0","28.0"]
["","Bypass mode","","Ultra high","dBA","27.0","28.0"]
["Heat exchange system","","","","","Air to air cross flow total heat (sensible + latent heat) exchange","Air to air cross flow total heat (sensible + latent heat) exchange"]
["Heat exchange element","","","","","Specially processed non-flammable paper","Specially processed non-flammable paper"]
["Connection duct diameter","mm","","","","100","150"]
["Operation mode","","","","","Heat exchange mode, bypass mode, fresh-up mode","Heat exchange mode, bypass mode, fresh-up mode"]
["SEC class","","","","","B, See note 4","B, See note 4"]
["Maximum flow rate at 100 Pa ESP","Flow rate","","","m³/h","130","207"]
["Sound power level (Lwa)","dB","","","","40","43"]
["Annual electricity consumption","kWh/a","","","","771","580"]
["Annual heating saved","Average climate","","","kWh/a","4571","4307"]
["","Cold climate","","","kWh/a","8941","8426"]
["","Warm climate","","","kWh/a","2067","1948"]
["Power supply","Name","","","","VE","VE"]
["","Phase","","","","1~","1~"]
["","Frequency","","","Hz","50/60","50/60"]
["","Voltage","","","V","220-240/220","220-240/220"]
["Notes","","","","","(1) - Measured according to JIS B 8628","(1) - Measured according to JIS B 8628"]
["","","","","","(2) - Measured at reference flow rate according to EN13141-7","(2) - Measured at reference flow rate according to EN13141-7"]
["","","","","","(3) - In accordance with commission regulation (EU) No 1254/2014","(3) - In accordance with commission regulation (EU) No 1254/2014"]
["","","","","","(4) - At reference flow rate in accordance with commission regulation (EU) No 1254/2014","(4) - At reference flow rate in accordance with commission regulation (EU) No 1254/2014"]